PDF4Java Reference Documentation
com.o2sol.pdf4java.spatial Package / PDFGeospatialMeasure Class
Collapse All Expand All Members Options: Show All Members Options: Filtered
Include Inherited Members
Include Protected Members
In This Topic

PDFGeospatialMeasure Class Methods
In This Topic

For a list of all members of this type, see PDFGeospatialMeasure members.

Public Methods

| Name | Description
--- | --- | ---
| getBounds | Gets the map bounds. For maps, this bounding polygon is known as a neatline. These points (x and y) are expressed relative to a unit square that describes the bounds associated with a , or .
| getCoordinateSystem | Gets the coordinate system.
| getCosMeasure | Gets the COS measure. (Inherited from com.o2sol.pdf4java.spatial.PDFMeasure)
| getDisplayCoordinateSystem | Gets the display coordinate system.
| getGeographicPoints | Gets the geographic points. These values shall be based on the geographic coordinate system described by .
| getLocalPoints | Gets the local points. The unit square is mapped to the rectangular bounds of the , or that contains the measure object. This array shall contain the same number of points as the array; each point is the unit square object position corresponding to the geospatial position in the array.
| getPreferredAngularDisplayUnit | Gets the preferred unit for displaying angles. Only these values are supported for this method: and .
| getPreferredAreaDisplayUnit | Gets the preferred unit for displaying areas. Only these values are supported for this method: , , , , and .
| getPreferredDistanceDisplayUnit | Gets the preferred unit for displaying distances. Only these values are supported for this method: , , , , and .
| setBounds | Sets the map bounds.
| setCoordinateSystem | Sets the coordinate system.
| setDisplayCoordinateSystem | Sets the display coordinate system.
| setGeographicPoints | Sets the geographic points. These values shall be based on the geographic coordinate system described by .
| setLocalPoints | Sets the local points. The unit square is mapped to the rectangular bounds of the , or that contains the measure object. This array shall contain the same number of points as the array; each point is the unit square object position corresponding to the geospatial position in the array.
| setPreferredAngularDisplayUnit | Sets the preferred unit for displaying angles. Only these values are supported for this method: and .
| setPreferredAreaDisplayUnit | Sets the preferred unit for displaying areas. Only these values are supported for this method: , , , , and .
| setPreferredDistanceDisplayUnit | Sets the preferred unit for displaying distances. Only these values are supported for this method: , , , , and .

Top
See Also

#### Reference

PDFGeospatialMeasure Class
com.o2sol.pdf4java.spatial Package

© 2025 O2 Solutions All Rights Reserved.

Send comments on this topic.